RMAX4 Tire/Fuel Carrier Install Instructions
Step 1
Install the two lower cage clamps directly above the weld on the bottom cage weldment pointing straight back.  Do not fully tighten the bolts yet as the clamps will need to be adjusted.
Step 2 
Measure the center to center distance of the heim joints on the carrier and adjust the bottom cage clamps to match.  Once adjusted install the carrier into the bottom clamps and install the outer half of the top clamps onto the carrier.  (Two people make this part much easier).
Step 3
With the top clamp halves installed on the carrier, push into position against the cage and install the back half of the clamp.  Do not fuly tighten the bolts as the clamps will need to be adjusted.
Step 4
Slowly start adjusting the clamps and tightening the bolts until the pins are easily removed and the vertical center to center distance of the clamps is equal to the vertical center to center distance of the carrier.  The heim joint position is preset but may require adjustment to get the pins to move easily.
Step 5
Once the clamps are fully tightened and while making sure the pins remain free, tighten the jam nuts on the heim joints.  Verify that all hardware is tight and the pins are still easily removed.

Thank you for purchasing this Dirt Road Fabrication product.  If you have questions please contact us at Dirtroadfabrication.com or 801-710-0910.